header format

(C)Copyright 2000 NTT Cyber Space Laboratories

member | type | value
channelMode | int | 0 (mono), 1(stereo)
Name | char[BUFSIZ] | character string (maximum length is BUFSIZ)
Comt | char[BUFSIZ] | character string (maximum length is BUFSIZ)
Auth | char[BUFSIZ] | character string (maximum length is BUFSIZ)
Cpyr | char[BUFSIZ] | character string (maximum length is BUFSIZ)
File | char[BUFSIZ] | character string (maximum length is BUFSIZ)
N_CAN_GLOBAL | int | 1, 2, 4, 8, 16, 32, the larger, the higher quality but slower encoder speed
ID | char[12] | TWIN97012000
samplingRate (kHz) | int |  | 8 | 11 | 16 | 22 | 44
bitRate (kbit/s) | int | mono | 8 | 8,10 | 16 | 20,24,32 | 40,48
stereo | 16 | 16,20 | 32 | 40,48,64 | 80,96
securityLevel | int | not used